{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":11,"rows_kept":21,"merged":[[0,5,0,10],[1,0,1,3],[1,5,1,10],[2,0,2,5],[2,6,2,10],[20,1,20,10]]}
["Date Submitted to Software Owner Responsible Line Manager (SRLM):",{"$nulls":4},"2017-04-10"]
["Submitted By (Name/Z# of Software Owner (SO):",{"$nulls":4},"James R. Smith/Z# 115119"]
["ESM Chapter 21 - Software, SOFT-GEN Section 2.0 Software Summary Required Fields",{"$nulls":5},"Optional Fields"]
["Summary Item No.","(a) Software Name","(b) Functional Description (What it does)","(c) Software Application \n(When/where/how it is used/or will be used at LANL)","(d) Can computer program be changed other than through replacement (Yes/No)?","(e) Is the software \"simple and easily understood\" software that will be individually verified each time the software is used (Yes/No)?","SRLM","Preliminary Associated ML (See Note 1)","Form 2033 completed (Yes/No)?","Other","Other"]
[1,"POSTMAX","Calculates the 95th percentile Maximally-Exposed Offsite Individual (MEOI) dispersion values from files of hourly  values generated by MACCS2 software.","Currently used LANL-wide to determine facility hazard categorization, associated controls and safety basis documentation for LANL facilities.","Yes","No","Tina Turner",1,"Yes (in 12/2016)"]
[{"$f":"A5+1","v":2},"CAESAR II","Performs pipe stress analysis, including static and dynamic analysis to measure the effects on a piping system from thermal, pressure, wind, seismic, etc. load.","Currently used for design and analysis of piping systems at TA-3 Power Plant which provides space heating to most of the buildings in TA-03.","No (software is Off-The-Shelf (OTS) software)","No","Tina Turner",4,"No (not planned; no \"reasonable probability\" per SOFT-GEN)"]
[{"$f":"A6+1","v":3},"SPOS","Shuts down electrical power to processes following a seismic event","Once purchased and installed, this software will be used to automatically shut down electrical power to processes in TA-55 Plutonium Facility (PF-4) laboratories following a seismic event.","No","No","Tina Turner",1,"No (but planned)"]
[4]
[5]
[6]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]
[15]
[]
["Notes:","1. This is the SO's best estimate of the highest management level (ML) of a facility SSC that is associated with the software.  Associated means that the software function is required for, and/or the software failure will have an adverse effect on the facility SSC."]